Copyright (C) 2002 Accton.
All rights reserved.
========================================================

Install Guide

This Document describes how to install ADM8515 Driver for MacOS X

1.Expend the file "ADM8515_X2v100.pkg.tgz"("ADM8515_X1v100b2.tgz" for X 10.1) by double click it.

2.Double click the program "ADM8515_X2v100.pkg"("ADM8515_X1.pkg" for X 10.1).

3.You should click the lock button and enter the administrator's user name and password. Then click the "Continue" button to continue the installation.  

4.The readme will be shown. Click the "Continue" button to continue.

5.The license information will be show.Click the continue botton. Then a popup window will be shown to ask you whether to agree. Click the "agree" button and the installation will be continued.

6.The installer will let you select a destination volume to install the driver.You should select the system volume and click the "continue" button.

7.Click the "install" button to perform installation. After you click the "install" button, a popup window will warn you the system need reboot after installation. you can click the canel button if you don't want to reboot the system. Otherwise, click the "continue installation" button.

8.When the install process completed, click the "reboot" button to reboot the system.
